4K IP Encoder

HD Encoder System Platform

中文 | English
System

- ◆ Input1 Status
- ◆ Input2 Status
- ◆ Input3 Status
- ◆ Input4 Status

## Status

###
Running Time:
Device Time:
(Sync Time To Device)
Device Name:
CPU Usage:
CPU Junction Temperature:
Memory Usage:

## WIFI

### WIFI:Disable

###
WIFI:
WIFI SSID:
WIFI IP:
WIFI MAC:
WIFI Level:
WIFI Freq:
WIFI Max Bit Rate:270 Mb/s

## Input1

Input status

###
Input Size:
Collected Video Frames:
Lost Video Frames:
Audio Samplerate:

Main Stream

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream1

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream2

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream3

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

## Input2

Input status

###
Input Size:
Collected Video Frames:
Lost Video Frames:
Audio Samplerate:

Main Stream

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream1

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream2

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream3

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

## Input3

Input status

###
Input Size:
Collected Video Frames:
Lost Video Frames:
Audio Samplerate:

Main Stream

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream1

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream2

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream3

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

## Input4

Input status

###
Input Size:
Collected Video Frames:
Lost Video Frames:
Audio Samplerate:

Main Stream

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream1

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream2

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)

Substream3

Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

###
Encoding Type:
Encoding Size:
Bitrate(kbit):
MJPG URL:
JPG URL:
TS URL:
HLS URL:
FLV URL:
RTSP URL:
RTMP URL:
RTMP PUSH URL:
Multicast URL:
SRT URL:
SRT PUSH URL:

Preview(Delay 2000ms)