4K IP Encoder

HD Encoder System Platform

中文 | English
Encoder

- ◆ Main Stream
- ◆ Substream1
- ◆ Substream2
- ◆ Substream3

OSD

- ◆ Main Stream
- ◆ Substream1
- ◆ Substream2
- ◆ Substream3
- ◆ Logo Upload

Video

- ◆ Video

Audio

- ◆ Audio

## Substream1

  Disabled (the main stream frame rate of 31~60 frames, will disable Substream)

Encoding Type:

FPS:
  [5-60]

GOP:
  [5-300]

Bitrate(kbit):
  [32-32000]

Image Quality Range:

Encoded Size:

H.264 Level:

Bitrate Control:

TS URL:

HLS URL:

FLV URL:

RTSP URL:

RTSP Multicast IP:

RTSP Multicast port:
  [1-65535]

RTMP URL:

RTMP(S)/RTSP PUSH URL:

Multicast IP:

Multicast prot:
  [1-65535]

SRT URL Port:
  [1-65535]

SRT PUSH URL:

SRT Encryption Password: