4K IP Encoder

HD Encoder System Platform

中文 | English
System

- ◆ Network
- ◆ WIFI
- ◆ 4G
- ◆ System

## System

Old Password:

New Password:

Confirm Password:

## Advanced

Device Name:

EDID:

Video Only:

Audio Only:

AV Sync Strategy:

Hls Splitter Time(s):
  [3-20]

Hls Number:
  [3-20]

SRT Latency(ms):
  [1-10000]

TS Muxer:

Net Drop Threshold:
  [50-50000]

Ts Once Pack:
  [3-128]

Ts_transport_stream_id:
  [1-65535]

Ts_pmt_start_pid:
  [16-7936]

Ts_start_pid:
  [32-3840]

Ts_tables_version:
  [0-31]

Ts_service_name:

Ts_service_provider:

TS Empty Packet:

TS Password Enable:

Vmix Compatible:

TS OVER RTSP:

Multicast Type:

UDP TTL:
  [1-254]

UDP SOCKET_BUF_SIZE:
  (0-20971520]

Slice Split Enable:

Slice Size:
  [128-65535]

MIN_QP:
  [1-35]

MAX_QP:
  (MIN_QP-50]

Contrast Improve:
  [0-63]

Image Enhance:
  [0-16]

Y Space Filter:
  [0-255]

Y Time Filter:
  [0-63]

C Space Filter:
  [0-255]

C Time Filter:
  [0-32]

## Schedule Restart

Restart Enable:

Restart Time:

## NTP

NTP Enable:

NTP Server:

Time Zone:

## Upload firmware and configuration

Select File:
  (File name is 'up.rar' or 'box.ini'. Please don't upload by different people at the same time, don't power off during upload.)

## Backup firmware and configuration

## System Settings